STELS ATV 800G GUEPARD in ST set is the most affordable ATV in GUEPARD family, maintaining excellent passability, safety and movement dynamics performances.

**Sturdy frame**

This model is based on a space frame made of steel pipes with a circular section. Verified design, ideal weight distribution and a high rigidity index are the key to the longevity for your chassis in all conditions. You can drive through the harsh terrain, overpass the ditches, scramble among the rocks and playfully fly off the spring-boards. This frame can handle all of these! Moreover, it’s covered with wear-resistant powder paint.

**Powerful two-cylinder engine**

ATV is equipped with a new two-cylinder V-shaped engine with a working volume of 800 cm3. Four-stroke engine has a power of 67 hp. Its maximum torque is about 73 Nm (available at 5000 rpm). The unit is equipped with an injection system (2 fuel injectors). It is allowed to fill in the 92 gasoline. The power pack start is accomplished by electric starter (breakerless ignition with electronic control). Despite the solid amount of volume and power, the engine is safely protected against overheating by the liquid-cooling system. The 800G GUEPARD ST fuel tank holds 29 l. Maximum speed is 140 km/h.

**Passability**

GUEPARD ST is an excellent choice for fishing and hunting trips in the remote areas. The ATV has a 32 cm ground clearance. Both front and rear suspensions are independent and have double wishbones. The stroke is 230 mm and 207 mm correspondingly. Spring-hydraulic shock-absorbers provide the excellent smoothness and protect from the breakdowns even on the complicated areas.

Transmission has a traditional utilitarian vehicle design: CVT V-belt variator, the front and the rear axles thrust is transmitted through the cardan shaft; locking of the front differential is provided as well. A pilot has a right to choose between the rear and the full wheel drive.

The model is thoroughly prepared to cope with any kind of water hazards. The fordable depth is restricted to the air-intake channel level (below the main body panel). The moisture entrapment from the air intake is performed by additional sediment bowls. Electric equipment, wiring, joints and a fuse panel are protected from the moisture as well, due to the 67 protection insulation class.

The ATV’s brake system is worthy of the highest praise. Unlike the other rivals, ATV 800G GUEPARD ST is serially equipped with disk brakes on all four wheels – one support per each. The driver can easily adjust brakes according to the need when driving down the steep slope.

**Comfort seating fit**

A special feature of the driver’s seat is a saddle with irregular hardness level. The rigidity varies from the center to the sides, providing an optimal weight distribution and allowing to spend more time driving without feeling any discomfort. Upholstery material is moisture-resistant. This material is resistant to extreme temperatures (hot or cold) and mechanical effect as well. Standard equipment includes a mirror and hand protective shields.

**Good original headlight**

Another GUEPARD’s advantage among the rivals is original headlights with LED crystals. It can ease the driving at night a lot. Besides, the vehicle is equipped with a LED stop lamp, LED side repeaters and position lights.

GUEPARD ST has been designed for one person; but it is also possible to position a passenger seat behind the driver. The back side of the vehicle is equipped with a luggage rack with a practical plastic cover.